Weather data collected by the Nature Conservancy and US Fish and Wildlife with the following instruments Logger: (2010-2016) Campbell Scientific, CR800 AirT and RH: (2010-2013) Vaisala, Model HMP45C (Oct 16 2010 to June 25 2013) AirT and RH: (2013-2016) Vaisala, Model HC2S3C (June 26 2013 to present) PAR: (2010-2014) Photosynthetically Active Radiation, Li-Cor, Model Li-190SB Barometric Pressure: (2010-2016) Setra, Model 278 (Campbell Scientific Model CS100) Rain Gage: (2010-2016) Met One, Model 380C Solar Panel: (2010-2016) BP Solar, Model SX310M Pyranometer: (2014-2016) Hukseflux LP02-00 (serial # 44837) Anemometer: (2015-2016) 03002 R.M. Young Wind Sentry Set (mod. 03101 anemometer; mod. 03301 wind vane)